**Build**

**Case Dimensions**

4 in. x 3 in.

**Screen Dimensions**

3 in. x 1 in.

20 x 4 Characters

**Electronics**

Rotary Encoder with Push Button

Push Button

ATmega328P Board

20 x 04 LCD

DS3231 Real-Time Clock Module

**Threading**

**Nut Size**

#4 – 40

**Bolt Size**

#4, 1 in.

**Code**

**Visit**

<https://github.com/Narwhalsss360/2004-clock>

**Clock**